**BD-10 Moisture Meter**

##### Features

1. Easy to read analog display
2. Two scales:
3. Wood Scale - 6% to 40% moisture range. Use for flooring and building material such as wood studs, floor joists, sub-floors
4. Reference Scale ­ reads from of 0 to 100 on a relative basis. Use on non-wood materials such as concrete, plaster, and insulation
5. Connector to attach external electrode
6. Rugged carrying case
7. 1 year warranty

The BD series, purchased individually, includes a carrying case and extra #2497/A-100 contact pins. Order as BD-10W/CS

The standard package includes a moisture meter, carrying case, #21-E electrode and extra #2497/A-100 contact pins. **Order as BD-10/PKG**

The 26 package includes the moisture meter, carrying case, #26-ES, and extra #496 and #2497/A-100 contact pins. **Order as BD-10/26/PKG**

The EIFS package includes the moisture meter, carrying case, #21-E electrode, (2) extra long 608-001 (6’’ penetration) pins, hole punch to make pilot holes, and extra #2497-A-100 pins. **Order as BD-10/EIFS/PKG**