**BDX-20 Moisture Meter**

##### Features

* Large, custom display with auto backlight - easy to read under all conditions
* Modern case design with large, tactile buttons and E-Z grip handle
* On-screen statistics for up to 100 readings saved to the meter
  + High, Low, Average, Standard Deviation
* Measuring Range:
  + Wood (Douglas Fir) 6%-60%
  + Drywall 0.1%-6%
  + Reference 1-100
* Wood temperature correction (°F / °C)
* Alarm set point - alerts to user-selected MC level
* Internal calibration check
* "Low Batt" warning with audio
* Auto off timer. Set to 1m, 4m or 10m
* Compatible with all Delmhorst electrodes

##### Meter Specifications

* Power: 2x AA Alkaline batteries
* Temperature Correction Range: 0°-255°F (-18°-124°C)
* QR code on meter for easy access to support materials and meter registration
* Size: meter only 8.65in x 2.85in x 1.60in
* (21.97cm x 7.24cm x 4.06cm)
* Weight: meter only - 8.6 (244gm)
* Hard plastic carrying case included
* 2-year warranty on manufacturer’s defects. Bonus warranty with on-line registration

The **BDX-20**, purchased individually, includes the BDX-20 meter, 324CAS-0111 carrying case, and two (2) spare 2498/A-100 pins. **Order as BDX-20W/CS**

The **Behind the Wall Package** includes the BDX-20 meter, 324CAS-0112 carrying case, 21-E electrode, and two (2) spare 2498/A-100 contact pins. **Order as BDX-20/P01**