**CX-30 Moisture Meter**

##### Features

* Large, custom display with auto backlight - easy to read under all conditions
* Modern case design with large, tactile buttons and
	+ E-Z grip handle
* On-screen statistics for up to 100 readings saved to the meter - High, Low, Average, Standard Deviation
* Measuring Ranges:
	+ Lint cotton (4%-18%)
	+ Seed cotton (6%-20%)
	+ Wool (12%-30%)
	+ Viscose/Rayon (6%-25%)
* Temperature correction (°F / °C)
* Bluetooth® connectivity to ***EDGE***® app
* Alarm set point – alerts to user-selected MC level
* Internal calibration check
* “Low Batt” warning with audio
* Auto off timer. Set to 1m, 4m or 10m
* Compatible with any Delmhorst electrode

##### Meter Specifications

* Power: 2x AA Alkaline batteries
* Temperature Correction Range: 0-255° F (-18-124°C)
* QR code on meter for easy access to support materials and meter registration
* Size: meter only - 8.03in x 2.85in x1.60in (20.40cm x 7.24cm x 4.06cm)
* Weight: meter only - 7.7oz (218gm)
* Hard plastic carrying case included
* 2-year warranty on manufacturer’s defects. Bonus warranty with on-line registration

**The Delmhorst *EDGE®* app**

* Timestamp and geotag
* Data export to .csv format
* Save unlimited readings

The **CX-30**, purchased individually, includes the CX-30 meter and 324CAS-0111 carrying case. **Order as CX-30W/CS**