**PX-20 Moisture Meter**

##### Features

* Large, custom display with auto backlight – easy to read under all conditions
* Modern case design with large, tactile buttons and E-Z grip handle
* On-screen statistics for up to 100 readings saved to the meter
	+ High, Low, Average, Standard Deviation
* Moisture Range: 4.3%-18% MC for paper (kraft paper calibration)
* Alarm set point - alerts to user-selected MC level
* Internal calibration check
* “Low Batt” warning with audio
* Auto off timer. Set to 1m, 4m or 10m
* Compatible with existing Delmhorst prods and electrodes

##### Meter Specifications

* Power: 2x AA Alkaline batter
* Temperature Correction Range: 0-255° F (-18-124°C)
* QR code on meter for easy access to support materials and meter registration
* Size: meter only - 8.65in x 2.85in x 1.60in (21.97cm x 7.24cm x 4.06cm)
* Weight: meter only - 8.6oz (244gm)
* Hard plastic carrying case included
* 2-year warranty on manufacturer’s defects. Bonus warranty with on-line registration

The **PX-20**, purchased individually, includes the PX-20 meter and 324CAS-0111 carrying Case. **Order as PX-20W/CS**

The **PX-20** **Package** includes the PX-20 meter and larger 324CAS-0112 carrying case. **Order as PX-20/P01**