**PX-30 Moisture Meter**

##### Features

* Large, custom display with auto backlight – easy to read under all conditions
* Modern case design with large, tactile buttons and E-Z grip handle
* On-screen statistics for up to 100 readings saved to the meter
	+ High, Low, Average, Standard Deviation
* Moisture Range:
	+ 4.3%-18% MC for paper (kraft paper calibration)
	+ 5%-40% for baled scrap paper
	+ 0 - 100 reference scale for obtaining relative moisture levels on other materials without calibration
* Temperature correction (°F / °C - PX-30 baled and scrap only)
* Bluetooth® connectivity to ***EDGE***® app
* Color-coded LEDs – adjustable through ***EDGE®*** app
* Alarm set point - alerts to user-selected MC level
* Internal calibration check
* “Low Batt” warning with audio
* Auto off timer. Set to 1m, 4m or 10m
* Compatible with existing Delmhorst prods and electrodes

##### Meter Specifications

* Power: 2x AA Alkaline batteries
* Temperature Correction Range: 0-255° F (-18-124°C)
* QR code on meter for easy access to support materials and meter registration
* Size: meter only - 8.65in x 2.85in x 1.60in (21.97cm x 7.24cm x 4.06cm)
* Weight: meter only - 8.6oz (244gm)
* Hard plastic carrying case included
* 2-year warranty on manufacturer’s defects. Bonus warranty with on-line registration

**The Delmhorst *EDGE®* app**

* Timestamp and geotag
* Data export to .csv format
* Save unlimited readings
* Customized LED ranges

The **PX-30**, purchased individually, includes the PX-30 meter and 324CAS-0111 carrying Case. **Order as PX-30W/CS**

The **PX-30** **Package** includes the PX-20 meter and larger 324CAS-0112 carrying case. **Order as PX-30/P01**

The **PX-30 Baled Package** includes the PX-30 meter and larger 324CAS-0112 carrying case, H-4 handle, and 830-2 10” prod. **Order as PX-30/P02**