**OVERVIEW**

Proscan is a noninvasive pinless moisture meter for flooring installers and inspectors who want to quickly find moisture in walls and floors. The non-invasive meter is made in the USA and uses radio frequency signals to quickly scan wood, drywall, concrete or other building materials without damaging the sample. Its built-in species corrections for woods with a specific gravity of between .30 and .80, checking a variety of wood species is a cinch. With ProScan professionals can work with confidence, save time, stay on budget and avoid call-backs.   
  
Add one to your tool box today!

**Features:**

* Handheld, compact, lightweight
* Easy-to-read digital display
* Quickly scan large areas to find moisture hot spots
* Calibrated to minimize false high readings
* Built-in battery/calibration checks
* Adjustable alarm alerts you when a preselected moisture level has been reached, allows the user to easily compare readings against an established dry standard
* Advanced RF technology makes it easy to quickly sweep large areas and locate high-moisture spots
* Hold function makes taking readings in hard-to-reach places fast and easy
* Built-in species corrections over the range of .30-.80 SG
* 0–100 reference scale for non-wood building materials
* Measures %MC on wood over the range of 5%–30%
* Rugged sensor pad measures moisture up to ¾" (1.9cm) deep without damaging the sample
* Size: 5-5/8” x 3-5/16” x 1-1/4”
* Weight: 8.5 oz.
* One 9-volt battery included
* Rugged carrying case
* 1-year warranty